Simulate in Simulink the system described from (2) to (11) in the attach file and evaluate the performance of a relay vs a PID controller working on the Pel control